2654 1734494294241 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is NOT null
2654 1734494294242 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9018, AttachedToolVID = 4d8
2654 1734494294242 GEN4_CONNECT_DIAGNOSTICS:transport type = USB
2654 1734494294242 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9018, AttachedToolVID = 4d8
2654 1734494294246 com.microchip.mplab.mdbcore.RealICETool.RIDbgToolCom
2654 1734494294246 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
2654 1734494294246 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
2654 1734494294246 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool.Connect() returned MPLABCOMM_NO_ERROR
2654 1734494294246 GEN4_CONNECT_DIAGNOSTICS:Attaching to MPLABCommTool plugnplay
2654 1734494294247 GEN4_CONNECT_DIAGNOSTICS:Adding new plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@2b3a1f7d
2654 1734494294247 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
2654 1734494294247 GEN4_CONNECT_DIAGNOSTICS:com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@2b3a1f7d
2654 1734494294247 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
2654 1734494294247 GEN4_CONNECT_DIAGNOSTICS:Registering for alternate PNP notifications. CommPnPCriteria.cPIDList = [9019, 901c, 2180], CommPnPCriteria.cSerialNumber = bur183076917

2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:init
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: Values:
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: pcAddress = 7fffffffffffffff, Vpp = 3.30, useRowEraseIfVoltageIsLow = false, voltageBelowWhichUseRowErase = 0.00, deviceName = ATSAMD21G18A, programmerType = NVMCTRL_U2207
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: MemInfo values:
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = ffffffff, exists = true, startAddr = 00000000, endAddr = 20007fff, rowSize = 0200, rowEraseSize = 0200, addrInc = 0004, widthProgram = 0004
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = ffffffff, exists = true, startAddr = 00804000, endAddr = 00804007, rowSize = 0001, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = ffffffff, exists = true, startAddr = 00804008, endAddr = 008040ff, rowSize = 0040, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0200, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = ffffffff, exists = true, startAddr = 40000000, endAddr = e000efff, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 7fffffff, exists = true, startAddr = 41002018, endAddr = 4100201b, rowSize = 0001, rowEraseSize = 0000, addrInc = 0001, widthProgram = 0001
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A CfgRequiredBitsMask Values:
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Address = 00804000, Mask = fe01ff77
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Address = 00804004, Mask = ffff01ff
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A BasicInfo: Values:
2654 1734494294305 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:init
2654 1734494294306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A none
2654 1734494294306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End

2654 1734494294306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:GetInterfaceProvider
2654 1734494294306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A RI4DebugInterface
2654 1734494294306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:GetInterfaceProvider
2654 1734494294306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A com.microchip.mplab.libs.RI4ToolsController.implementations.RI4DebugInterfaceImpl@3c2e689a
2654 1734494294306 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End

2654 1734494294308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:GetInterfaceProvider
2654 1734494294308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A RI4ProgramInterface
2654 1734494294308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:GetInterfaceProvider
2654 1734494294308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ProgramInterfaceImpl@41031d75
2654 1734494294308 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End

2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:GetInterfaceProvider
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A RI4ConnectInterface
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:GetInterfaceProvider
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A com.microchip.mplab.libs.PK4ToolsController.PK4ConnectInterfaceImpl@7d668ea4
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End
2654 1734494294310 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9018, 9019, 901c]
2654 1734494294310 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2180]
2654 1734494294310 GEN4_CONNECT_DIAGNOSTICS:Setting selected tool type to pk4
2654 1734494294310 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2180]
2654 1734494294310 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9018, 9019, 901c]

2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:GetInterfaceProvider
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A RI4ControllerDiagnosticsInterface
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:GetInterfaceProvider
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ControllerDiagnosticsInterfaceImpl@2457dcc8
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End

2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:GetInterfaceProvider
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A ProgrammerToGo
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:GetInterfaceProvider
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A com.microchip.mplab.libs.RI4ToolsController.implementations.ProgrammerToGoImpl@1c72ba5a
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End

2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:GetInterfaceProvider
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Status
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:GetInterfaceProvider
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A null
2654 1734494294310 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End
2654 1734494294312 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
2654 1734494294312 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@3e22ccc3
2654 1734494294312 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:uMode = checkingVersions
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:Parsing file  for firmware updates
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ParseSelectedVersionsFromJamFile()
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_boot.hex,010155
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:Jame file line = scripts.xml,000849
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app1 020286, 0040C000
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app2 1.11.20, 00500000
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app3 000000, FFFFFFFF
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app4 000000, FFFFFFFF
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app5 000000, FFFFFFFF
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app6 000000, FFFFFFFF
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app7 000000, FFFFFFFF
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app8 000000, FFFFFFFF
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ri4ParseSelectedVersionsFromJamFile()
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
2654 1734494294313 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4

2654 1734494294313 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:EstablishCommunincations
2654 1734494294313 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294313 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A com.microchip.mplab.mdbcore.PK4Tool.PK4Com@65cbcc81
2654 1734494294313 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294313 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:EstablishCommunincations
2654 1734494294313 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294313 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A true
2654 1734494294313 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2654 1734494294313 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetFirmwareInfo
2654 1734494294313 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294313 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2654 1734494294313 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294320 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetFirmwareInfo
2654 1734494294320 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294320 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: Values:
2654 1734494294320 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: boot = false, bootVer = 01.01.55, apVer = 02.02.86, fpgaVer = ff.ff.ff, scriptVer = 00.08.49, macAddress = 0495583547050515048485152484952, devID = a1020e01, devID1 = 1, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR183076917, appCommitID = null, scriptCommitID = 6cc6313c7b, PCB_ID = 1
2654 1734494294320 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End
2654 1734494294323 GEN4_CONNECT_DIAGNOSTICS:appNeedsUpdate returned false
2654 1734494294323 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

2654 1734494294323 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:EstablishCommunincations
2654 1734494294323 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294323 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A com.microchip.mplab.mdbcore.PK4Tool.PK4Com@65cbcc81
2654 1734494294323 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294325 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:EstablishCommunincations
2654 1734494294325 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294325 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A true
2654 1734494294325 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2654 1734494294325 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetFirmwareInfo
2654 1734494294325 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294325 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2654 1734494294325 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294332 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetFirmwareInfo
2654 1734494294332 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294332 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: Values:
2654 1734494294332 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: boot = false, bootVer = 01.01.55, apVer = 02.02.86, fpgaVer = ff.ff.ff, scriptVer = 00.08.49, macAddress = 0495583547050515048485152484952, devID = a1020e01, devID1 = 1, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR183076917, appCommitID = null, scriptCommitID = 6cc6313c7b, PCB_ID = 1
2654 1734494294332 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2654 1734494294332 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetFirmwareInfo
2654 1734494294332 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294332 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2654 1734494294332 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294339 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetFirmwareInfo
2654 1734494294339 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294339 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: Values:
2654 1734494294339 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: boot = false, bootVer = 01.01.55, apVer = 02.02.86, fpgaVer = ff.ff.ff, scriptVer = 00.08.49, macAddress = 0495583547050515048485152484952, devID = a1020e01, devID1 = 1, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR183076917, appCommitID = null, scriptCommitID = 6cc6313c7b, PCB_ID = 1
2654 1734494294339 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End
2654 1734494294339 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
2654 1734494294339 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@3e22ccc3
2654 1734494294340 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
2654 1734494294340 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
2654 1734494294340 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
2654 1734494294340 GEN4_CONNECT_DIAGNOSTICS:uMode = done
2654 1734494294340 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
2654 1734494294340 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
2654 1734494294340 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
2654 1734494294340 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
2654 1734494294340 GEN4_CONNECT_DIAGNOSTICS:Don't upgrade fimware = false
2654 1734494294340 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
2654 1734494294340 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
2654 1734494294340 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

2654 1734494294340 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:SetPowerInfo
2654 1734494294340 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294340 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A PowerInfo: Values:
2654 1734494294340 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A PowerInfo: shotDownSystem = false, isToolPower = false, voltage = 3.300000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
2654 1734494294340 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294340 XXXX 1734494294340, Thread 2654: XXXX 1734494294340, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
2654 1734494294343 XXXX 1734494294343, Thread 2654: XXXX 1734494294343, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294343 XXXX 1734494294343, Thread 2654: XXXX 1734494294343, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
2654 1734494294344 XXXX 1734494294344, Thread 2654: XXXX 1734494294344, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294344 XXXX 1734494294344, Thread 2654: XXXX 1734494294344, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
2654 1734494294345 XXXX 1734494294345, Thread 2654: XXXX 1734494294345, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294345 XXXX 1734494294345, Thread 2654: XXXX 1734494294345, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0xef, ...  
2654 1734494294346 XXXX 1734494294346, Thread 2654: XXXX 1734494294346, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294346 XXXX 1734494294346, Thread 2654: XXXX 1734494294346, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
2654 1734494294347 XXXX 1734494294347, Thread 2654: XXXX 1734494294347, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294347 XXXX 1734494294347, Thread 2654: XXXX 1734494294347, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
2654 1734494294348 XXXX 1734494294348, Thread 2654: XXXX 1734494294348, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294348 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:SetPowerInfo
2654 1734494294348 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294348 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A none
2654 1734494294348 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2654 1734494294348 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetVoltageInfo
2654 1734494294348 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294348 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2654 1734494294348 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294348 XXXX 1734494294348, Thread 2654: XXXX 1734494294348, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
2654 1734494294349 XXXX 1734494294349, Thread 2654: XXXX 1734494294349, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294349 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetVoltageInfo
2654 1734494294349 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294349 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A VoltagesInfo: Values:
2654 1734494294349 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A VoltagesInfo: internalVdd = 3300, internalVpp = 3300, targetVdd = 3300, targetVpp = 3300, vddSense = 3300, temp = 25000, vddCurrentSense = 0, vddVoltageSense = 3300
2654 1734494294349 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2654 1734494294349 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetFirmwareInfo
2654 1734494294349 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294349 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2654 1734494294349 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294358 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetFirmwareInfo
2654 1734494294358 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294358 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: Values:
2654 1734494294358 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: boot = false, bootVer = 01.01.55, apVer = 02.02.86, fpgaVer = ff.ff.ff, scriptVer = 00.08.49, macAddress = 0495583547050515048485152484952, devID = a1020e01, devID1 = 1, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR183076917, appCommitID = null, scriptCommitID = 6cc6313c7b, PCB_ID = 1
2654 1734494294358 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2654 1734494294358 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:SetToolInfo
2654 1734494294358 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294358 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A ToolInfo: Values:
2654 1734494294358 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A ToolInfo: speedLevel = 1, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
2654 1734494294358 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294358 XXXX 1734494294358, Thread 2654: XXXX 1734494294358, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
2654 1734494294361 XXXX 1734494294361, Thread 2654: XXXX 1734494294361, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294361 XXXX 1734494294361, Thread 2654: XXXX 1734494294361, Entering Thread 2654: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
2654 1734494294363 XXXX 1734494294363, Thread 2654: XXXX 1734494294363, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294363 XXXX 1734494294363, Thread 2654: XXXX 1734494294363, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
2654 1734494294364 XXXX 1734494294364, Thread 2654: XXXX 1734494294364, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294364 XXXX 1734494294364, Thread 2654: XXXX 1734494294364, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0x3b, ...  
2654 1734494294365 XXXX 1734494294365, Thread 2654: XXXX 1734494294365, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294365 XXXX 1734494294365, Thread 2654: XXXX 1734494294365, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
2654 1734494294366 XXXX 1734494294366, Thread 2654: XXXX 1734494294366, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294366 XXXX 1734494294366, Thread 2654: XXXX 1734494294366, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
2654 1734494294367 XXXX 1734494294367, Thread 2654: XXXX 1734494294367, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294367 XXXX 1734494294367, Thread 2654: XXXX 1734494294367, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
2654 1734494294368 XXXX 1734494294368, Thread 2654: XXXX 1734494294368, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294368 XXXX 1734494294368, Thread 2654: XXXX 1734494294368, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
2654 1734494294369 XXXX 1734494294369, Thread 2654: XXXX 1734494294369, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294369 XXXX 1734494294369, Thread 2654: XXXX 1734494294369, Entering Thread 2654: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
2654 1734494294370 XXXX 1734494294370, Thread 2654: XXXX 1734494294370, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494294370 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:SetToolInfo
2654 1734494294370 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494294370 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A none
2654 1734494294370 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2654 1734494294370 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetTargetIDInfo
2654 1734494294370 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2654 1734494294370 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2654 1734494294370 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2654 1734494294372 XXXX 1734494294372, Thread 2654: XXXX 1734494294372, Entering Thread 2654: Commands::runScriptBasic, script name = InitSWD, timeOut = -1 ms  
2654 1734494295406 XXXX 1734494295406, Thread 2654: XXXX 1734494295406, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494295406 XXXX 1734494295406, Thread 2654: XXXX 1734494295406, Entering Thread 2654: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
2654 1734494295408 XXXX 1734494295408, Thread 2654: XXXX 1734494295408, Exiting Thread 2654: Commands::runScriptBasic  
2654 1734494295408 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetTargetIDInfo
2654 1734494295408 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2654 1734494295408 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A TargetIDInfo: Values:
2654 1734494295408 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A TargetIDInfo: DeviceID = 00211805
2654 1734494295408 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End
2588 1734494298678 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is null

2588 1734494298678 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetFirmwareInfo
2588 1734494298678 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2588 1734494298678 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2588 1734494298678 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2588 1734494298686 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetFirmwareInfo
2588 1734494298686 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2588 1734494298686 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: Values:
2588 1734494298686 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: boot = false, bootVer = 01.01.55, apVer = 02.02.86, fpgaVer = ff.ff.ff, scriptVer = 00.08.49, macAddress = 0495583547050515048485152484952, devID = a1020e01, devID1 = 1, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR183076917, appCommitID = null, scriptCommitID = 6cc6313c7b, PCB_ID = 1
2588 1734494298686 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2588 1734494298686 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:SetPowerInfo
2588 1734494298686 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2588 1734494298686 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A PowerInfo: Values:
2588 1734494298686 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A PowerInfo: shotDownSystem = false, isToolPower = false, voltage = 3.300000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
2588 1734494298686 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2588 1734494298686 XXXX 1734494298686, Thread 2588: XXXX 1734494298686, Entering Thread 2588: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
2588 1734494298687 XXXX 1734494298687, Thread 2588: XXXX 1734494298687, Exiting Thread 2588: Commands::runScriptBasic  
2588 1734494298687 XXXX 1734494298687, Thread 2588: XXXX 1734494298687, Entering Thread 2588: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
2588 1734494298688 XXXX 1734494298688, Thread 2588: XXXX 1734494298688, Exiting Thread 2588: Commands::runScriptBasic  
2588 1734494298688 XXXX 1734494298688, Thread 2588: XXXX 1734494298688, Entering Thread 2588: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
2588 1734494298689 XXXX 1734494298689, Thread 2588: XXXX 1734494298689, Exiting Thread 2588: Commands::runScriptBasic  
2588 1734494298689 XXXX 1734494298689, Thread 2588: XXXX 1734494298689, Entering Thread 2588: Commands::runScriptBasic with script contents. contents[0] = 0xef, ...  
2588 1734494298690 XXXX 1734494298690, Thread 2588: XXXX 1734494298690, Exiting Thread 2588: Commands::runScriptBasic  
2588 1734494298690 XXXX 1734494298690, Thread 2588: XXXX 1734494298690, Entering Thread 2588: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
2588 1734494298691 XXXX 1734494298691, Thread 2588: XXXX 1734494298691, Exiting Thread 2588: Commands::runScriptBasic  
2588 1734494298691 XXXX 1734494298691, Thread 2588: XXXX 1734494298691, Entering Thread 2588: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
2588 1734494298692 XXXX 1734494298692, Thread 2588: XXXX 1734494298692, Exiting Thread 2588: Commands::runScriptBasic  
2588 1734494298692 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:SetPowerInfo
2588 1734494298692 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2588 1734494298692 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A none
2588 1734494298692 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End
2588 1734494298692 GEN4_CONNECT_DIAGNOSTICS:Removing plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@2b3a1f7d
2588 1734494298692 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
2588 1734494298692 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
2588 1734494298743 GEN4_CONNECT_DIAGNOSTICS:Calling RIDbgToolCom.Disconnect
2588 1734494298743 GEN4_CONNECT_DIAGNOSTICS:Calling MPLABCommTool.Detach to remove tool from plug and play list
2588 1734494298743 GEN4_CONNECT_DIAGNOSTICS:Calling RIDbgToolCom.DisconnectFromMPlabComm
2588 1734494298743 GEN4_CONNECT_DIAGNOSTICS:Calling MPLABCommTool.Disconnect
2666 1734494304695 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool is NOT null
2666 1734494304695 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9018, AttachedToolVID = 4d8
2666 1734494304695 GEN4_CONNECT_DIAGNOSTICS:transport type = USB
2666 1734494304695 GEN4_CONNECT_DIAGNOSTICS:AttachedToolPID = 9018, AttachedToolVID = 4d8
2666 1734494304698 com.microchip.mplab.mdbcore.RealICETool.RIDbgToolCom
2666 1734494304698 GEN4_CONNECT_DIAGNOSTICS:Before MPLABCommTool.Connect()
2666 1734494304698 GEN4_CONNECT_DIAGNOSTICS:After MPLABCommTool.Connect()
2666 1734494304698 GEN4_CONNECT_DIAGNOSTICS:MPLABCommTool.Connect() returned MPLABCOMM_NO_ERROR
2666 1734494304698 GEN4_CONNECT_DIAGNOSTICS:Attaching to MPLABCommTool plugnplay
2666 1734494304698 GEN4_CONNECT_DIAGNOSTICS:Adding new plug and play observer com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@a325a30
2666 1734494304698 GEN4_CONNECT_DIAGNOSTICS:Begin PlugNPlayObservers list dump:
2666 1734494304698 GEN4_CONNECT_DIAGNOSTICS:com.microchip.mplab.mdbcore.RI4Tool.RI4ToolBase$RI4PlugNPlayObserver@a325a30
2666 1734494304698 GEN4_CONNECT_DIAGNOSTICS:End PlugNPlayObservers list dump:
2666 1734494304698 GEN4_CONNECT_DIAGNOSTICS:Registering for alternate PNP notifications. CommPnPCriteria.cPIDList = [9019, 901c, 2180], CommPnPCriteria.cSerialNumber = bur183076917

2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:init
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: Values:
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: pcAddress = 7fffffffffffffff, Vpp = 3.30, useRowEraseIfVoltageIsLow = false, voltageBelowWhichUseRowErase = 0.00, deviceName = ATSAMD21G18A, programmerType = NVMCTRL_U2207
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: MemInfo values:
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = ffffffff, exists = true, startAddr = 00000000, endAddr = 20007fff, rowSize = 0200, rowEraseSize = 0200, addrInc = 0004, widthProgram = 0004
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = ffffffff, exists = true, startAddr = 00804000, endAddr = 00804007, rowSize = 0001, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = ffffffff, exists = true, startAddr = 00804008, endAddr = 008040ff, rowSize = 0040, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0200, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = ffffffff, exists = true, startAddr = 40000000, endAddr = e000efff, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0004, widthProgram = 0004
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 7fffffff, exists = true, startAddr = 41002018, endAddr = 4100201b, rowSize = 0001, rowEraseSize = 0000, addrInc = 0001, widthProgram = 0001
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A DeviceInfo: mask = 0000, exists = false, startAddr = 00000000, endAddr = 00000000, rowSize = 0000, rowEraseSize = 0000, addrInc = 0000, widthProgram = 0000
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A CfgRequiredBitsMask Values:
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Address = 00804000, Mask = fe01ff77
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Address = 00804004, Mask = ffff01ff
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A BasicInfo: Values:
2666 1734494304728 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:init
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A none
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End

2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:GetInterfaceProvider
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A RI4DebugInterface
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:GetInterfaceProvider
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A com.microchip.mplab.libs.RI4ToolsController.implementations.RI4DebugInterfaceImpl@29539d1
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End

2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:GetInterfaceProvider
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A RI4ProgramInterface
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:GetInterfaceProvider
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ProgramInterfaceImpl@16071f91
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End

2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:GetInterfaceProvider
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A RI4ConnectInterface
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:GetInterfaceProvider
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A com.microchip.mplab.libs.PK4ToolsController.PK4ConnectInterfaceImpl@e7c24bb
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End
2666 1734494304729 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9018, 9019, 901c]
2666 1734494304729 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2180]
2666 1734494304729 GEN4_CONNECT_DIAGNOSTICS:Setting selected tool type to pk4
2666 1734494304729 GEN4_CONNECT_DIAGNOSTICS:otherPIDs = [2180]
2666 1734494304729 GEN4_CONNECT_DIAGNOSTICS:acceptablePIDs = [9018, 9019, 901c]

2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:GetInterfaceProvider
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A RI4ControllerDiagnosticsInterface
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:GetInterfaceProvider
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A com.microchip.mplab.libs.RI4ToolsController.implementations.RI4ControllerDiagnosticsInterfaceImpl@18d7894c
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End

2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:GetInterfaceProvider
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A ProgrammerToGo
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:GetInterfaceProvider
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A com.microchip.mplab.libs.RI4ToolsController.implementations.ProgrammerToGoImpl@33277036
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End

2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Pre:GetInterfaceProvider
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Status
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Post:GetInterfaceProvider
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A null
2666 1734494304729 GEN4_TO_CONTROLLER_LOG:GEN4_INIT_INT_LOG_ATSAMD21G18A Return End
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@1df21a54
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:uMode = checkingVersions
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:Parsing file  for firmware updates
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ParseSelectedVersionsFromJamFile()
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_boot.hex,010155
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:Jame file line = scripts.xml,000849
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app1 020286, 0040C000
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app2 1.11.20, 00500000
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app3 000000, FFFFFFFF
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app4 000000, FFFFFFFF
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app5 000000, FFFFFFFF
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app6 000000, FFFFFFFF
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app7 000000, FFFFFFFF
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:Jame file line = snap_app8 000000, FFFFFFFF
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.ri4ParseSelectedVersionsFromJamFile()
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.GetUpdateInfo()
2666 1734494304731 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4

2666 1734494304731 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:EstablishCommunincations
2666 1734494304731 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304731 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A com.microchip.mplab.mdbcore.PK4Tool.PK4Com@5bbd2dc3
2666 1734494304731 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304731 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:EstablishCommunincations
2666 1734494304731 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304731 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A true
2666 1734494304731 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2666 1734494304731 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetFirmwareInfo
2666 1734494304731 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304731 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2666 1734494304731 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304738 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetFirmwareInfo
2666 1734494304738 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304738 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: Values:
2666 1734494304738 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: boot = false, bootVer = 01.01.55, apVer = 02.02.86, fpgaVer = ff.ff.ff, scriptVer = 00.08.49, macAddress = 0495583547050515048485152484952, devID = a1020e01, devID1 = 1, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR183076917, appCommitID = null, scriptCommitID = 6cc6313c7b, PCB_ID = 1
2666 1734494304738 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End
2666 1734494304741 GEN4_CONNECT_DIAGNOSTICS:appNeedsUpdate returned false
2666 1734494304741 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

2666 1734494304741 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:EstablishCommunincations
2666 1734494304741 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304741 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A com.microchip.mplab.mdbcore.PK4Tool.PK4Com@5bbd2dc3
2666 1734494304741 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304742 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:EstablishCommunincations
2666 1734494304742 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304742 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A true
2666 1734494304742 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2666 1734494304742 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetFirmwareInfo
2666 1734494304742 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304742 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2666 1734494304742 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304748 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetFirmwareInfo
2666 1734494304748 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304748 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: Values:
2666 1734494304748 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: boot = false, bootVer = 01.01.55, apVer = 02.02.86, fpgaVer = ff.ff.ff, scriptVer = 00.08.49, macAddress = 0495583547050515048485152484952, devID = a1020e01, devID1 = 1, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR183076917, appCommitID = null, scriptCommitID = 6cc6313c7b, PCB_ID = 1
2666 1734494304748 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2666 1734494304748 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetFirmwareInfo
2666 1734494304748 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304748 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2666 1734494304748 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304755 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetFirmwareInfo
2666 1734494304755 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304755 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: Values:
2666 1734494304755 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: boot = false, bootVer = 01.01.55, apVer = 02.02.86, fpgaVer = ff.ff.ff, scriptVer = 00.08.49, macAddress = 0495583547050515048485152484952, devID = a1020e01, devID1 = 1, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR183076917, appCommitID = null, scriptCommitID = 6cc6313c7b, PCB_ID = 1
2666 1734494304755 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:Created FirmwareUpdateHandler com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler@1df21a54
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:areWeInBoot returned false
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:inBoot = false
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:uMode = done
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:selectedTool = pk4
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:current toolType = pk4
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:current tool mode = pk4
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:Don't upgrade fimware = false
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:ENTERING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.updatePk4HybridFirmware()
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.pk4hybrid.pk4hybridFirmwareUpdateHandler.UpdateFirmware(FirmwareInfo, UpdateMessage)
2666 1734494304756 GEN4_CONNECT_DIAGNOSTICS:EXITING: com.microchip.mplab.mdbcore.RI4Tool.ConnectionHandler.CheckForFWUpdates()

2666 1734494304756 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:SetPowerInfo
2666 1734494304756 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304756 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A PowerInfo: Values:
2666 1734494304756 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A PowerInfo: shotDownSystem = false, isToolPower = false, voltage = 3.300000, useVppFirst = false, useLowVoltageProgramming = true, useMaintainActivePower = false
2666 1734494304756 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304756 XXXX 1734494304756, Thread 2666: XXXX 1734494304756, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0x39, ...  
2666 1734494304757 XXXX 1734494304757, Thread 2666: XXXX 1734494304757, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304757 XXXX 1734494304757, Thread 2666: XXXX 1734494304757, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0x46, ...  
2666 1734494304758 XXXX 1734494304758, Thread 2666: XXXX 1734494304758, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304758 XXXX 1734494304758, Thread 2666: XXXX 1734494304758, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0x44, ...  
2666 1734494304759 XXXX 1734494304759, Thread 2666: XXXX 1734494304759, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304759 XXXX 1734494304759, Thread 2666: XXXX 1734494304759, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0xef, ...  
2666 1734494304760 XXXX 1734494304760, Thread 2666: XXXX 1734494304760, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304760 XXXX 1734494304760, Thread 2666: XXXX 1734494304760, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0x40, ...  
2666 1734494304761 XXXX 1734494304761, Thread 2666: XXXX 1734494304761, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304761 XXXX 1734494304761, Thread 2666: XXXX 1734494304761, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
2666 1734494304762 XXXX 1734494304762, Thread 2666: XXXX 1734494304762, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304762 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:SetPowerInfo
2666 1734494304762 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304762 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A none
2666 1734494304762 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2666 1734494304762 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetVoltageInfo
2666 1734494304762 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304762 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2666 1734494304762 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304762 XXXX 1734494304762, Thread 2666: XXXX 1734494304762, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0x47, ...  
2666 1734494304763 XXXX 1734494304763, Thread 2666: XXXX 1734494304763, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304763 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetVoltageInfo
2666 1734494304763 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304763 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A VoltagesInfo: Values:
2666 1734494304763 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A VoltagesInfo: internalVdd = 3300, internalVpp = 3300, targetVdd = 3300, targetVpp = 3300, vddSense = 3300, temp = 25000, vddCurrentSense = 0, vddVoltageSense = 3300
2666 1734494304763 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2666 1734494304763 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetFirmwareInfo
2666 1734494304763 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304763 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2666 1734494304763 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304770 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetFirmwareInfo
2666 1734494304770 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304770 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: Values:
2666 1734494304770 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A FirmwareInfo: boot = false, bootVer = 01.01.55, apVer = 02.02.86, fpgaVer = ff.ff.ff, scriptVer = 00.08.49, macAddress = 0495583547050515048485152484952, devID = a1020e01, devID1 = 1, devSN0 = ffffffff, devSN1 = ffffffff, serialNumber = BUR183076917, appCommitID = null, scriptCommitID = 6cc6313c7b, PCB_ID = 1
2666 1734494304770 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2666 1734494304770 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:SetToolInfo
2666 1734494304770 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304770 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A ToolInfo: Values:
2666 1734494304770 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A ToolInfo: speedLevel = 1, PGCResistance = 4700, PGDResistance = 4700, PGCPullDir = PullDown, PGDPullDir = PullDown, ICSPSelected = Wire2
2666 1734494304770 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304770 XXXX 1734494304770, Thread 2666: XXXX 1734494304770, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0x27, ...  
2666 1734494304771 XXXX 1734494304771, Thread 2666: XXXX 1734494304771, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304771 XXXX 1734494304771, Thread 2666: XXXX 1734494304771, Entering Thread 2666: Commands::runScriptBasic, script name = SetSpeedFromDevice, timeOut = -1 ms  
2666 1734494304772 XXXX 1734494304772, Thread 2666: XXXX 1734494304772, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304772 XXXX 1734494304772, Thread 2666: XXXX 1734494304772, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0xed, ...  
2666 1734494304773 XXXX 1734494304773, Thread 2666: XXXX 1734494304773, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304773 XXXX 1734494304773, Thread 2666: XXXX 1734494304773, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0x3b, ...  
2666 1734494304774 XXXX 1734494304774, Thread 2666: XXXX 1734494304774, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304774 XXXX 1734494304774, Thread 2666: XXXX 1734494304774, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0xd4, ...  
2666 1734494304775 XXXX 1734494304775, Thread 2666: XXXX 1734494304775, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304775 XXXX 1734494304775, Thread 2666: XXXX 1734494304775, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
2666 1734494304776 XXXX 1734494304776, Thread 2666: XXXX 1734494304776, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304776 XXXX 1734494304776, Thread 2666: XXXX 1734494304776, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
2666 1734494304777 XXXX 1734494304777, Thread 2666: XXXX 1734494304777, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304777 XXXX 1734494304777, Thread 2666: XXXX 1734494304777, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0xcd, ...  
2666 1734494304778 XXXX 1734494304778, Thread 2666: XXXX 1734494304778, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304778 XXXX 1734494304778, Thread 2666: XXXX 1734494304778, Entering Thread 2666: Commands::runScriptBasic with script contents. contents[0] = 0xce, ...  
2666 1734494304779 XXXX 1734494304779, Thread 2666: XXXX 1734494304779, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494304779 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:SetToolInfo
2666 1734494304779 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494304779 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A none
2666 1734494304779 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2666 1734494304779 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Pre:GetTargetIDInfo
2666 1734494304779 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload
2666 1734494304779 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A null
2666 1734494304779 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Payload End
2666 1734494304781 XXXX 1734494304781, Thread 2666: XXXX 1734494304781, Entering Thread 2666: Commands::runScriptBasic, script name = InitSWD, timeOut = -1 ms  
2666 1734494305815 XXXX 1734494305815, Thread 2666: XXXX 1734494305815, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494305815 XXXX 1734494305815, Thread 2666: XXXX 1734494305815, Entering Thread 2666: Commands::runScriptBasic, script name = GetDeviceID, timeOut = -1 ms  
2666 1734494305816 XXXX 1734494305816, Thread 2666: XXXX 1734494305816, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494305816 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Post:GetTargetIDInfo
2666 1734494305816 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return Value
2666 1734494305816 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A TargetIDInfo: Values:
2666 1734494305816 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A TargetIDInfo: DeviceID = 00211805
2666 1734494305816 GEN4_TO_CONTROLLER_LOG:GEN4_CONNECT_INT_LOG_ATSAMD21G18A Return End

2666 1734494307343 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A Pre:SendOperation
2666 1734494307343 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A Payload
2666 1734494307343 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A OperationInfo: Values:
2666 1734494307343 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A OperationInfo: Type = erase, Mask = 00000000, Erase = false, Production Mode = true
2666 1734494307343 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A TransferInfo: Start = 0, End = 3ffff, Buffer Length = 0, Type = Pgm, Mask = 00000000
2666 1734494307343 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A TransferInfo: Start = 804000, End = 804007, Buffer Length = 0, Type = Cfg, Mask = 00000000
2666 1734494307343 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A TransferInfo: Start = 804008, End = 8040ff, Buffer Length = 0, Type = UserID, Mask = 00000000
2666 1734494307343 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A TransferInfo: Start = 20000000, End = 20007fff, Buffer Length = 0, Type = FileRegs, Mask = 00000000
2666 1734494307343 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A Payload End
2666 1734494307343 XXXX 1734494307343, Thread 2666: XXXX 1734494307343, Entering Thread 2666: Commands::runScriptBasic, script name = EraseChip, timeOut = -1 ms  
2666 1734494307344 XXXX 1734494307344, Thread 2666: XXXX 1734494307344, Exiting Thread 2666: Commands::runScriptBasic  
2666 1734494307344 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A Post:SendOperation
2666 1734494307344 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A Return Value
2666 1734494307344 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A None
2666 1734494307344 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A Return End

2666 1734494307344 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A Pre:SendOperation
2666 1734494307344 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A Payload
2666 1734494307344 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A OperationInfo: Values:
2666 1734494307344 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A OperationInfo: Type = read, Mask = 00000000, Erase = false, Production Mode = true
2666 1734494307344 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A TransferInfo: Start = 804000, End = 8040ff, Buffer Length = 256, Type = Cfg, Mask = 00000002
2666 1734494307344 GEN4_TO_CONTROLLER_LOG:GEN4_PROGRAM_INT_LOG_ATSAMD21G18A Payload End
2666 1734494307344 XXXX 1734494307344, Thread 2666: XXXX 1734494307344, Entering Thread 2666: Commands::runScriptWithUpload, script name = ReadConfigmem  
2666 1734494307344 XXXX 1734494307344, Thread 2666: XXXX 1734494307344, Entering Thread 2666: ToolCommUsb::readTransfer, sideData is 0x24 bytes long, transferDataLength is 0x100 bytes long  
2673 1734494321378 XXXX 1734494321378, Thread 2673: ToolCommUsb::read, com.Received returned -1 
2666 1734494321378 XXXX 1734494321378, Thread 2666: com.Send returned false 
2673 1734494321380 XXXX 1734494321380, Thread 2673: ToolCommUsb::DataReader::run, fatal RI4ControllerException: {null} 
